

SUZUKI GSXR1000 L1-2015 SLIP ON EXHAUST

CUT OFF STOCK LINK PIPE AFTER CAT AS SHOWN

CLAMP ON NEW LINK PIPE

BOLT UP TO REAR OF FOOTREST IN 1 OF 2 HOLES USING SUPPLIED WHITE SPACER, WASHER AND BOLT